Skip to main content
`Ctrl`+`K`

# scipy.signal.buttord

scipy.signal.buttord(wp, ws, gpass, gstop, analog=False, fs=None)

  Butterworth filter order selection.

  Return the order of the lowest order digital or analog Butterworth filter that loses no more than gpass dB in the passband and has at least gstop dB attenuation in the stopband.

  Parameters:
    wp, ws float

      Passband and stopband edge frequencies.

      For digital filters, these are in the same units as fs. By default, fs is 2 half-cycles/sample, so these are normalized from 0 to 1, where 1 is the Nyquist frequency. (wp and ws are thus in half-cycles / sample.) For example:

      > - Lowpass: wp = 0.2, ws = 0.3

      > - Highpass: wp = 0.3, ws = 0.2

      > - Bandpass: wp = [0.2, 0.5], ws = [0.1, 0.6]

      > - Bandstop: wp = [0.1, 0.6], ws = [0.2, 0.5]

      For analog filters, wp and ws are angular frequencies (e.g., rad/s).

    gpass float

      The maximum loss in the passband (dB).

    gstop float

      The minimum attenuation in the stopband (dB).

    analog bool, optional

      When True, return an analog filter, otherwise a digital filter is returned.

    fs float, optional

      The sampling frequency of the digital system.

      New in version 1.2.0.

  Returns:
    ord int

      The lowest order for a Butterworth filter which meets specs.

    wn ndarray or float

      The Butterworth natural frequency (i.e. the “3dB frequency”). Should be used with `butter` to give filter results. If fs is specified, this is in the same units, and fs must also be passed to `butter`.

  See also

  `butter`

    Filter design using order and critical points

  `cheb1ord`

    Find order and critical points from passband and stopband spec

  `cheb2ord`, `ellipord`
  `iirfilter`

    General filter design using order and critical frequencies

  `iirdesign`

    General filter design using passband and stopband spec

  Examples

  Design an analog bandpass filter with passband within 3 dB from 20 to 50 rad/s, while rejecting at least -40 dB below 14 and above 60 rad/s. Plot its frequency response, showing the passband and stopband constraints in gray.

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt
      >>> import numpy as np

      >>> N, Wn = signal.buttord([20, 50], [14, 60], 3, 40, True)
      >>> b, a = signal.butter(N, Wn, 'band', True)
      >>> w, h = signal.freqs(b, a, np.logspace(1, 2, 500))
      >>> plt.semilogx(w, 20 * np.log10(abs(h)))
      >>> plt.title('Butterworth bandpass filter fit to constraints')
      >>> plt.xlabel('Frequency [radians / second]')
      >>> plt.ylabel('Amplitude [dB]')
      >>> plt.grid(which='both', axis='both')
      >>> plt.fill([1,  14,  14,   1], [-40, -40, 99, 99], '0.9', lw=0) # stop
      >>> plt.fill([20, 20,  50,  50], [-99, -3, -3, -99], '0.9', lw=0) # pass
      >>> plt.fill([60, 60, 1e9, 1e9], [99, -40, -40, 99], '0.9', lw=0) # stop
      >>> plt.axis([10, 100, -60, 3])
      >>> plt.show()