Skip to main content
`Ctrl`+`K`

# scipy.signal.cspline1d_eval

scipy.signal.cspline1d_eval(cj, newx, dx=1.0, x0=0)

  Evaluate a cubic spline at the new set of points.

  dx is the old sample-spacing while x0 was the old origin. In other-words the old-sample points (knot-points) for which the cj represent spline coefficients were at equally-spaced points of:

  > oldx = x0 + j*dx j=0…N-1, with N=len(cj)

  Edges are handled using mirror-symmetric boundary conditions.

  Parameters:
    cj ndarray

      cublic spline coefficients

    newx ndarray

      New set of points.

    dx float, optional

      Old sample-spacing, the default value is 1.0.

    x0 int, optional

      Old origin, the default value is 0.

  Returns:
    res ndarray

      Evaluated a cubic spline points.

  See also

  `cspline1d`

    Compute cubic spline coefficients for rank-1 array.

  Examples

  We can filter a signal to reduce and smooth out high-frequency noise with a cubic spline:

      >>> import numpy as np
      >>> import matplotlib.pyplot as plt
      >>> from scipy.signal import cspline1d, cspline1d_eval
      >>> rng = np.random.default_rng()
      >>> sig = np.repeat([0., 1., 0.], 100)
      >>> sig += rng.standard_normal(len(sig))*0.05  # add noise
      >>> time = np.linspace(0, len(sig))
      >>> filtered = cspline1d_eval(cspline1d(sig), time)
      >>> plt.plot(sig, label="signal")
      >>> plt.plot(time, filtered, label="filtered")
      >>> plt.legend()
      >>> plt.show()