Skip to main content
`Ctrl`+`K`

# scipy.signal.ShortTimeFFT.fs

property ShortTimeFFT.fs

  Sampling frequency of input signal and of the window.

  The sampling frequency is the inverse of the sampling interval `T`. A `ValueError` is raised if it is set to a non-positive value.

  See also

  `delta_t`

    Time increment of STFT (`hop*T`)

  `hop`

    Time increment in signal samples for sliding window.

  `T`

    Sampling interval of input signal and of the window (`1/fs`).

  `ShortTimeFFT`

    Class this property belongs to.