Skip to main content
`Ctrl`+`K`

# scipy.signal.hilbert

scipy.signal.hilbert(x, N=None, axis=-1)

  Compute the analytic signal, using the Hilbert transform.

  The transformation is done along the last axis by default.

  Parameters:
    x array_like

      Signal data. Must be real.

    N int, optional

      Number of Fourier components. Default: `x.shape[axis]`

    axis int, optional

      Axis along which to do the transformation. Default: -1.

  Returns:
    xa ndarray

      Analytic signal of x, of each 1-D array along axis

  Notes

  The analytic signal `x_a(t)` of signal `x(t)` is:

  \[x_a = F^{-1}(F(x) 2U) = x + i y\]

  where F is the Fourier transform, U the unit step function, and y the Hilbert transform of x. [1]

  In other words, the negative half of the frequency spectrum is zeroed out, turning the real-valued signal into a complex signal. The Hilbert transformed signal can be obtained from `np.imag(hilbert(x))`, and the original signal from `np.real(hilbert(x))`.

  References

  [1]

  Wikipedia, “Analytic signal”. https://en.wikipedia.org/wiki/Analytic_signal

  [2]

  Leon Cohen, “Time-Frequency Analysis”, 1995. Chapter 2.

  [3]

  Alan V. Oppenheim, Ronald W. Schafer. Discrete-Time Signal Processing, Third Edition, 2009. Chapter 12. ISBN 13: 978-1292-02572-8

  Examples

  In this example we use the Hilbert transform to determine the amplitude envelope and instantaneous frequency of an amplitude-modulated signal.

      >>> import numpy as np
      >>> import matplotlib.pyplot as plt
      >>> from scipy.signal import hilbert, chirp

      >>> duration = 1.0
      >>> fs = 400.0
      >>> samples = int(fs*duration)
      >>> t = np.arange(samples) / fs

  We create a chirp of which the frequency increases from 20 Hz to 100 Hz and apply an amplitude modulation.

      >>> signal = chirp(t, 20.0, t[-1], 100.0)
      >>> signal *= (1.0 + 0.5 * np.sin(2.0*np.pi*3.0*t) )

  The amplitude envelope is given by magnitude of the analytic signal. The instantaneous frequency can be obtained by differentiating the instantaneous phase in respect to time. The instantaneous phase corresponds to the phase angle of the analytic signal.

      >>> analytic_signal = hilbert(signal)
      >>> amplitude_envelope = np.abs(analytic_signal)
      >>> instantaneous_phase = np.unwrap(np.angle(analytic_signal))
      >>> instantaneous_frequency = (np.diff(instantaneous_phase) /
      ...                            (2.0*np.pi) * fs)

      >>> fig, (ax0, ax1) = plt.subplots(nrows=2)
      >>> ax0.plot(t, signal, label='signal')
      >>> ax0.plot(t, amplitude_envelope, label='envelope')
      >>> ax0.set_xlabel("time in seconds")
      >>> ax0.legend()
      >>> ax1.plot(t[1:], instantaneous_frequency)
      >>> ax1.set_xlabel("time in seconds")
      >>> ax1.set_ylim(0.0, 120.0)
      >>> fig.tight_layout()