'

# Latency Test

From Audacity Development Manual
Latency refers to the delay between the time the audio enters the computer and the time Audacity is able to record it to a track. For example, if you are recording a keyboard track, latency is the delay between the time you strike a key and the time that note is recorded.

| Latency correction is only "set and forget" if you always use the same recording device, the same sound system, the same sample rate ... every time that you record. If that is not the case then latency correction should be tested and set each time that you record, if there\'s a chance that you may use a feature that requires it to be set.

## When latency adjustment is important

Latency is only important when you are using:

- overdubbing, that is, recording a new track while listening to previously-recorded track(s). You want what you play to be in sync with the tracks you are listening to. Audacity can correct for latency, but you have to tell it what the correction amount is. You enter this correction amount in the Devices tab of the Preferences dialog
- Punch and Roll Record to quick-fix recording errors.

## What you need

### Using a microphone

If you are using a microphone to record overdubs then the loop-back cable method will not work for you. Instead you need to set up the microphone in front of a speaker or headphones! Don\'t worry, you will not get feedback because you\'ve turned Software Playthrough off.

  Example of loopback using a microphone

### Using a laptop computer\'s on-board microphone

You can just, straightforwardly, use the laptop\'s onboard microphone and speaker(s) for the latency test, if that is what you are planning to use for subsequent recording.

### Using a desk-top computer

To use a desk-top computer you will need to connect the line input and line output ports on the computer, using a loop-back cable. The type of cable you need will depend on the way you are connecting your recording equipment to the computer.

If you are connecting your recording equipment to the line input and line output jacks on your computer you need a cable with a stereo mini-plug at each end.

  A stereo loop-back cable | A loop-back cable plugged in

### Using an external USB audio interface

If you are not using the line input and/or line output ports on your computer but are instead using a USB audio interface device for input and/or output, plug the loop-back cable into the appropriate jacks on the USB interface.

Depending on your interface you may need a different type of loop-back cable.

  Example of loopback with a USB audio adapter

| Note that using a USB microphone is not the best way to record overdubs. These microphones are great for podcasters who just want to record their voice and are not worried about syncing to music. The problem with these microphones is that the only way you can hear yourself in your headphones is by turning Software Playthrough On. Software playthrough introduces its own delay (different from latency) which you will hear in your headphones. Tests on the same system used for the latency test below revealed that the Software Playthrough delay was 65 milliseconds. This does not sound like much, but it is like hearing your voice coming out of speakers 70 feet away. If you are serious about overdubbing, get an inexpensive mixer and a good microphone to go with it. For more information on overdubbing with Audacity, see our Tutorial - Recording Multi-track Overdubs

## Making the necessary settings

### Recording preferences

Click on Edit > Preferences.

On the Recording tab, set the following settings:

- Play other tracks while recording (overdub) checked.
- Software playthrough of input not checked.

| In Audacity by default using the Record button will append record onto your existing track, see the Recording page. In order to record on a new track, for multi-track overdubbing, you will need to use Shift and the Record New track button , or use its shortcut Shift + R. You can change this in Recording Preferences by checking "on" the "Record on a new track", doing this will make Audacity record on a new track with just the Record button and Shift and will append record onto your existing track.

### Devices preferences

On the Devices tab, in the Latency section, set the following settings:

- Set the Latency compensation to 0 (zero), so that you get an absolute reading.
- Leave the Buffer length value at its default value.
- Click OK.

| The Buffer length value will affect latency, but the effect will vary between systems. 100 milliseconds is a safe value that will not put too much load on the CPU. Too low a value may put too much load on the CPU causing dropouts in the recording. If you are feeling adventurous you can repeat this test with different values for Buffer length. But in the end you should settle on a value for both Buffer length and Latency compensation and leave them there.

### Selection toolbar

In Selection Toolbar make sure that "Snap-To" is set to "Off". Above the second and thrid group of numbers, make sure that Beginning and Length of Selection is selected. Click on one of the downward-pointing arrows in the digits boxes to the right of Snap-To and select hh:mm:ss + milliseconds .

## Doing the latency test

Turn off un-necessary applications before starting the test so that the computer can mostly concentrate on playing and recording the audio.

Click on Generate > Rhythm Track. Set "Number of Measures (bars)" to 2, and set the "Beat Sound" to Ping . Click OK to generate the click track. Make sure the first track is completely selected (if you do nothing, it will be completely selected).

Now press Shift and click the Record new track button in the Transport Toolbar - the rhythm track will be played back and recorded on a new track. You will now have something like this:

  The top track is the original click track, the bottom track is the looped-back recording. Note the delay.

Zoom in so you can see one of the clicks in the top track and its delayed version on the bottom track.

Using Selection Tool, drag a selection starting at the start of the click in the top track and ending at the start of the delayed click in the second track.

You should see something like this (your numbers are likely to be different):

  The selections go from the original click to the delayed version in the bottom track.

You can now read the latency directly from the second panel of numbers. In this case it is 0.096 seconds, or 96 milliseconds.

Click on Edit > Preferences, click on the Devices tab, and enter the negative of this number in the Latency compensation box - in this case it would be -96.

## Checking the result

Delete the second track by clicking the close box X in its Track Control Panel.

Click the Fit to Width button to see the entire click track. Click in the Track Control Panel of the remaining track to select it, then click the Record button.

After the recording is finished Audacity will apply the latency Correction by pushing the newly-recorded track back by the Latency Correction amount.

Note the two arrows at the left end of the second track - they are warning you that latency correction has been applied and part of the recorded track has been pushed left so that it starts before 0 seconds. This is OK, it is what we wanted to happen. The arrows are there to remind you that latency correction has been applied, just in case that is not what you wanted.

  Note the arrows at left end of recorded track: latency correction has been applied with the track moved backwards.

Zoom in on one of the clicks and verify that the clicks in the two tracks line up.

  Note that there is still a tiny delay between the two tracks

You will never get it absolutely perfect. In this case we are still off by 17 samples. At 44100 samples per second that is about 0.39 milliseconds.

This is as close as we are going to get, and it is not an audible difference. This is the length of time it takes a sound wave to travel about 5 inches, and the latency will probably have natural variability greater than this each time you record.

However if you really need to, you can set the latency correction amount to a fraction of a millisecond (for example -96.4).

## If you change recording or playback devices or audio host

If you change any of your recording or playback (for example, if you change from using the line input port on your computer to using a USB audio interface) or if you use the same device but change the Audio Host in Device Toolbar, then you will need to do this test again. The test you just did only applies for the specific inputs and outputs and host used during the test. Equally you should record for real with as many other applications shut down as possible, which was the scenario in which you did the test.

'