Skip to main content
`Ctrl`+`K`

# scipy.signal.ShortTimeFFT.T

property ShortTimeFFT.T

  Sampling interval of input signal and of the window.

  A `ValueError` is raised if it is set to a non-positive value.

  See also

  `delta_t`

    Time increment of STFT (`hop*T`)

  `hop`

    Time increment in signal samples for sliding window.

  `fs`

    Sampling frequency (being `1/T`)

  `t`

    Times of STFT for an input signal with n samples.

  `ShortTimeFFT`

    Class this property belongs to.